|  |  |
| --- | --- |
| variables |  |
| Bolt Size | M12 |
| M16 |
| Preload Level | 100% |
| 75% |
| 50% |
| 25% |
| Bolt Type | Normal |
| Blind |
| Loadings | Static, Monotonic |
| Cyclic, Vibration |
| Connection Type | Double-Lap Joint |
| Single-Lap Joint |